{"text_format":"1","workbook":"xlsx","n_sheets":3,"sheets":["偏心補正計算","γ","XYZ2φλh"],"not_rendered":{"charts":0,"images":2,"macros":1,"external_links":0,"defined_names":3,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"偏心補正計算","index":0,"n_rows":38,"n_cols":9,"rows_kept":38,"cut":false,"hidden":false,"merged":[[0,0,0,7],[1,0,1,1]]}
["偏心補正計算",null,null,null,null,null,null,null,"©武市測量事務所"]
["(既知点の偏心)",null,null,null,null,null,null,null,"https://canuta.sakura.ne.jp/takeitchisurveyoffice/"]
["入力点=C","点名","(304)Ⅳ岡"]
[null,"緯度",35.355765640000001,"φ"]
[null,"経度",138.39123610999999,"λ"]
[null,"楕円体高",497.94,"h"]
[]
[null,"X",-3898082.8470505099]
[null,"Y",3430166.7330274954]
[null,"Z",3692426.1460538195]
[]
[null,"偏心測定距離",15.032999999999999,"D'","m1=",1.5,"g2=",1.6]
[null,"測定高度角(C～B)",-3.2204000000000002,"α1'","i1=",1.5,"f2=",1.6]
[null,"測定高度角(B～C)",3.22,"α2'","i2=",1.6,"f1=",1.5]
[]
[]
[null,"偏心距離",15.039204850159901,"D"]
[null,"偏心高度角(C～B)",-3.4453155522684327,"α1"]
[null,"偏心高度角(B～C)",3.4449157084910129,"α2"]
[null,"平均偏心高度角",-3.445115630379723,"αm"]
[]
[null,"零方向の方位角",350.48103099999997,"T0（GNSS観測記簿より）"]
[null,"偏心角",246.07480000000001,"θ（TS観測手簿より）"]
[null,"方位角(B～C)",236.55583099999998,"T=T0+θ"]
[null,"方位角(C～B)",56.555801918145896,"T'=T±180°-γ"]
[]
[null,"Δx=",-4.1297690793254684]
[null,"Δy=",-13.118203815001362]
[null,"Δz=",6.0856732203269139]
[]
["計算測点=B","緯度",35.355792205750923]
[null,"経度",138.39128606882244]
[null,"楕円体高",496.95705001801252]
[null,"直交座標X",-3898086.9768195893]
[null,"直交座標Y",3430153.6148236804]
[null,"直交座標Z",3692432.2317270399]
[]
[null,null,"(注)角度の入力方法は「d.ms」とする。"]

{"sheet":"γ","index":1,"n_rows":22,"n_cols":6,"rows_kept":22,"cut":false,"hidden":false,"merged":[]}
["本点から偏心点の方位角計算",null,null,null,null,"©武市測量事務所"]
["T",236.55583099999998,"偏心点から既知点の方位角",null,null,"https://canuta.sakura.ne.jp/takeitchisurveyoffice/"]
["T'0",56.555830999999984,"既知点から偏心点の方位角(初期値)"]
["T'",56.555801918145896,"既知点から偏心点の方位角"]
["γ",2.9081854092118713E-5,"偏心点における子午線収差角"]
["S'",15.005875294077835,"基準面上の距離"]
["D",15.039204850159901,"既知点と偏心点の斜距離"]
["φ1",35.355765640000001,"既知点の緯度"]
["φC",35.355792205724889]
["X",8.1875262350683506]
["NC",6385383.5469307071,"卯酉線曲率半径（引数はφCとする）"]
["M",6357057.899979867,"子午線曲率半径（引数はφ1とする）"]
["R",6371204.9688724605,"平均曲率半径（引数はφ1とする）"]
["α1",-3.4453155522684327,"既知点の高低角"]
["α2",3.4449157084910129,"偏心点の高低角"]
["αm",-3.445115630379723,"平均高低角"]
["h1",497.94,"本点の楕円体高"]
["h2",496.95705006457865,"偏心点の楕円体高"]
["hm",497.44852503228935,"平均楕円体高"]
["a",6378137,"長半径(GRS80)"]
["b",6356752.3141403561,"短半径(GRS80)"]
["1/f",298.25722210100002,"扁平率(GRS80)の逆数"]

{"sheet":"XYZ2φλh","index":2,"n_rows":13,"n_cols":6,"rows_kept":13,"cut":false,"hidden":false,"merged":[]}
["地心直交座標から緯度・経度・楕円体高への換算",null,null,null,null,"©武市測量事務所"]
["X",-3898086.9768195893,"地心直交座標",null,null,"https://canuta.sakura.ne.jp/takeitchisurveyoffice/"]
["Y",3430153.6148236804,"〃"]
["Z",3692432.2317270399,"〃"]
["φ",35.355792205750923,"緯度"]
["λ",138.39128606882244,"経度"]
["h",496.95705001801252,"楕円体高"]
["P",5192401.7467967989]
["N",6385383.5469307322,"卯酉線曲率半径"]
["a",6378137,"長半径(GRS80)"]
["b",6356752.3141403561,"短半径(GRS80)"]
["1/f",298.25722210100002,"扁平率(GRS80)の逆数"]
["e",8.1819191042815168E-2,"第一離心率"]